Dear Kind Human(s) with amazing eyesight and steady hands,

Enclosed please find

* three Phidget Single Board Computers (only two need changes)
* three 30pf capacitors (you only need two)
* Instructions

The Phidget SBC labeled 22 and marked as Good No Changes came with the fix applied. No changes need to be made. Use as a reference

The Phidget SBCs labeled 21 and 23 need the 30pf capacitors applied as described in the attached instructions. I have placed a piece of blue tape with an arrow to indicate where (I think) the caps go.

Using SBC 22 as a reference, remove the covers from SBC 21 and SBC 23 and apply one 30pf capacitor to each.

I really appreciate your help. Buy yourself / friends something to celebrate the holdays.

Good Everything,

Christopher

(949)540-4431

[chrhodes@cox.net](mailto:chrhodes@cox.net)

p.s. If you are wondering what the heck these are used for, picture Halloween Skulls moved with small servo motors. Lot’s of fun.